# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of Cleaning Equipment p 1 /…**

**Publication reference:** 08-655/2

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments onits proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | 1 small size truck with upgrade suitable for collection of waste in narrow streets; EURO 6 with OBD step E; Engine power minimum 110 kW (150 HP); Engine capacity minimum 2800 cm3; Axles 4X2; Distance of the axles maximum 3400 mm; Total payload maximum 7500 kg; Seats 3 including driver; Tank capacity minimum 100 l; Warranty at least 36 months. |  |  |  |
| **2** | 5 petrol grass trimmers; Engine capacity minimum 35 cm3; Engine power minimum 1,5 kW; Maximum weight 7,5 kg; Standard head with possibility of blade replacement and change. Warranty at least 12 months. |  |  |  |
| **3** | 1 petrol ride-on lawn mower; 2 cylinders engine minimum capacity 600 cm3; minimum power 8,5 kW; Single pedal self propulsion; Cutting width minimum 100 cm; cutting height from 30 to 100 mm; Grass catcher box minimum 320 l; Fuel tank capacity minimum 8,5 l; Warranty at least 12 months. |  |  |  |
|  |  |  |  |  |